| ## SDI Interface
Move the mouse accross the display elements to get the corresponding descriptions.
The SDI Interface instrument displays the relevant parameters of a mounted 3G-SDI Deembedder Interface. If valid signals with valid audio groups are present in the SDI data stream, deembedding is performed and their status will be displayed on the SDI Interface instrument. Then, the decoded AES signal pairs are available for the input routing of the TouchMonitor.