| ## ISA - Immersive Sound Analyzer
Example: 5.1.4 Immersive Format (5.1 in Main Bed, 4.0 in Upper Bed) Move the mouse accross the display elements to get the corresponding descriptions.
The display of the Immersive Sound Analyzer supports 5.1.2, 5.1.4, 7.1.2 or 7.1.4 formats, exists of two layers (beds) and is based on the functionality of the Surround Sound Analyzer. The display refers to the loudness like ITU BS.1770 (k) or other weighting filters. It equates to the listening sound pressure level, when the units and the studio monitoring system are properly calibrated. The axes of the 45° rotated coordinate system use dB SPL, LKFS, LU, or LUFS scales, with a reference mark that is also shown in the loudness and SPL displays in the Program Meter. The cyan lines, whose ends move on the axes and form a rectangle depending on the level in the individual channels, represent the total volume of the Main Bed (middle layer) of the immersive format, the orange-colored lines the total volume of the Upper Bed (upper layer). An important element is the Immersive Dominance Indicator, which as a white dot represents the relationship between the two levels and shows the position and height of the entire signal. If the dot is larger and closer to the orange X (Dominance Indicator of the Upper Bed), the subjectively perceived spatial focal point is more in the Upper Bed. If the dot is smaller and closer to the cyan + (Dominance Indicator of the Main Bed), the focal point is more in the Main Bed.
Further information and examples about reading the graphical display provides the interactive demonstration of the elements of SSA.